Login authentication

Username:
#Easy-Operation: Stop upgrading because of the input in the console.
#Easy-Operation: Enter the status of running normally.
Username:admin
Password:
Warning: The default password poses security risks.
The password needs to be changed. Change now? [Y/N]: y
Please enter old password:
Please enter new password:
Please confirm new password:
The password has been changed successfully.
Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommend                                                                  ed version information.
<HUAWEI>sys
Enter system view, return user view with Ctrl+Z.
[HUAWEI]sysname LSW2
[LSW2]
Nov 30 2024 13:29:31 LSW2 DS/4/DATASYNC_CFGCHANGE:OID 1.3.6.1.4.1.2011.5.25.191.                                                                  3.1 configurations have been changed. The current change number is 212, the chan                                                                  ge loop count is 0, and the maximum number of records is 4095.
[LSW2]un in en
Info: Information center is disabled.
[LSW2]int et
[LSW2]int Eth-Trunk 1
[LSW2-Eth-Trunk1]mode la
[LSW2-Eth-Trunk1]mode lacp
[LSW2-Eth-Trunk1]q
[LSW2]int g0/0/3
[LSW2-GigabitEthernet0/0/3]rth
[LSW2-GigabitEthernet0/0/3]et
[LSW2-GigabitEthernet0/0/3]eth-trunk 1
Info: This operation may take a few seconds. Please wait a moment.
Info: The operation is successful.
[LSW2-GigabitEthernet0/0/3]int g0/0/4
[LSW2-GigabitEthernet0/0/4]eth-trunk 1
Info: This operation may take a few seconds. Please wait a moment.
Info: The operation is successful.
[LSW2-GigabitEthernet0/0/4]int g0/0/5
[LSW2-GigabitEthernet0/0/5]eth-trunk 1
Info: This operation may take a few seconds. Please wait a moment.
Info: The operation is successful.
[LSW2-GigabitEthernet0/0/5]q
[LSW2]vlan bat
[LSW2]vlan batch 10 20
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW2]int g0/0/1
[LSW2-GigabitEthernet0/0/1]port link
[LSW2-GigabitEthernet0/0/1]port link-t
[LSW2-GigabitEthernet0/0/1]port link-type acc
[LSW2-GigabitEthernet0/0/1]port link-type access
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW2-GigabitEthernet0/0/1]i
[LSW2-GigabitEthernet0/0/1]int g0/0/2
[LSW2-GigabitEthernet0/0/2]port link-type access
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW2-GigabitEthernet0/0/2]int g0/0/3
[LSW2-GigabitEthernet0/0/3]port link-
[LSW2-GigabitEthernet0/0/3]int g0/0/6
[LSW2-GigabitEthernet0/0/6]port lin
[LSW2-GigabitEthernet0/0/6]port link-t
[LSW2-GigabitEthernet0/0/6]port link-type tru
[LSW2-GigabitEthernet0/0/6]port link-type trunk
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW2-GigabitEthernet0/0/6]undo port lin
[LSW2-GigabitEthernet0/0/6]undo port link-t
[LSW2-GigabitEthernet0/0/6]undo port link-type tru
[LSW2-GigabitEthernet0/0/6]undo port link-type tru
                                               ^
Error:Too many parameters found at '^' position.
[LSW2-GigabitEthernet0/0/6]undo port link-type
[LSW2-GigabitEthernet0/0/6]dis eth
[LSW2-GigabitEthernet0/0/6]dis eth-trunk 1
Eth-Trunk1's state information is:
Local:
LAG ID: 1                   WorkingMode: LACP
Preempt Delay: Disabled     Hash arithmetic: According to SIP-XOR-DIP
System Priority: 32768      System ID: 6012-3c9a-61f0
Least Active-linknumber: 1  Max Active-linknumber: 8
Operate status: up          Number Of Up Port In Trunk: 2
--------------------------------------------------------------------------------
ActorPortName          Status   PortType PortPri PortNo PortKey PortState Weight
GigabitEthernet0/0/3   Selected 1GE      32768   1      305     10111100  1
GigabitEthernet0/0/4   Selected 1GE      32768   2      305     10111100  1
GigabitEthernet0/0/5   Unselect 1GE      32768   3      305     10110000  1

Partner:
--------------------------------------------------------------------------------
ActorPortName          SysPri   SystemID        PortPri PortNo PortKey PortState
GigabitEthernet0/0/3   100      642c-acc1-65e0  100     1      305     10111100
GigabitEthernet0/0/4   100      642c-acc1-65e0  100     2      305     10111100
GigabitEthernet0/0/5   100      642c-acc1-65e0  32768   3      305     10100000

[LSW2-GigabitEthernet0/0/6]

User interface con0 is available

Please Press ENTER.

Login authentication

Username:admin
Password:
Info: Lastest accessed IP: Invalid IP address  Time: 2024-11-30 13:29:07  Failed: 0

Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW2>sys
Enter system view, return user view with Ctrl+Z.
[LSW2]disp vlan
The total number of VLANs is: 3
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
1    common  UT:GE0/0/1(U)      GE0/0/2(U)      GE0/0/6(D)      GE0/0/7(D)
                GE0/0/8(D)      GE0/0/9(D)      GE0/0/10(D)     GE0/0/11(D)
                GE0/0/12(D)     GE0/0/13(D)     GE0/0/14(D)     GE0/0/15(D)
                GE0/0/16(D)     GE0/0/17(D)     GE0/0/18(D)     GE0/0/19(D)
                GE0/0/20(D)     GE0/0/21(D)     GE0/0/22(D)     GE0/0/23(D)
                GE0/0/24(D)     GE0/0/25(D)     GE0/0/26(D)     GE0/0/27(D)
                GE0/0/28(D)     Eth-Trunk1(U)
10   common  TG:Eth-Trunk1(U)
20   common  TG:Eth-Trunk1(U)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
1    enable  default       enable  disable    VLAN 0001
10   enable  default       enable  disable    VLAN 0010
20   enable  default       enable  disable    VLAN 0020
[LSW2]

User interface con0 is available

Please Press ENTER.

Login authentication

Username:admin
Password:
Info: Lastest accessed IP: Invalid IP address  Time: 2024-11-30 14:01:03  Failed: 0

Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW2>ping 192.168.10.1
  PING 192.168.10.1: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out
    Request time out
    Request time out
    Request time out

  --- 192.168.10.1 ping statistics ---
    5 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

<LSW2>ping 192.168.10.3
  PING 192.168.10.3: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out
    Request time out
    Request time out
    Request time out

  --- 192.168.10.3 ping statistics ---
    5 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

<LSW2>ping 192.168.10.1
  PING 192.168.10.1: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out
    Request time out
    Request time out
    Request time out

  --- 192.168.10.1 ping statistics ---
    5 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

<LSW2>ping 192.168.10.1
  PING 192.168.10.1: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out

  --- 192.168.10.1 ping statistics ---
    2 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

<LSW2>ping 192.168.10.3
  PING 192.168.10.3: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out
    Request time out
    Request time out

  --- 192.168.10.3 ping statistics ---
    4 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

<LSW2>sys
Enter system view, return user view with Ctrl+Z.
[LSW2]dis port vlan
Port                        Link Type    PVID  Trunk VLAN List
-------------------------------------------------------------------------------
Eth-Trunk1                  auto         1     1-4094
GigabitEthernet0/0/1        access       1     -
GigabitEthernet0/0/2        access       1     -
GigabitEthernet0/0/3        -            0     -
GigabitEthernet0/0/4        -            0     -
GigabitEthernet0/0/5        -            0     -
GigabitEthernet0/0/6        auto         1     1-4094
GigabitEthernet0/0/7        auto         1     1-4094
GigabitEthernet0/0/8        auto         1     1-4094
GigabitEthernet0/0/9        auto         1     1-4094
GigabitEthernet0/0/10       auto         1     1-4094
GigabitEthernet0/0/11       auto         1     1-4094
GigabitEthernet0/0/12       auto         1     1-4094
GigabitEthernet0/0/13       auto         1     1-4094
GigabitEthernet0/0/14       auto         1     1-4094
GigabitEthernet0/0/15       auto         1     1-4094
GigabitEthernet0/0/16       auto         1     1-4094
GigabitEthernet0/0/17       auto         1     1-4094
GigabitEthernet0/0/18       auto         1     1-4094
GigabitEthernet0/0/19       auto         1     1-4094
GigabitEthernet0/0/20       auto         1     1-4094
GigabitEthernet0/0/21       auto         1     1-4094
GigabitEthernet0/0/22       auto         1     1-4094
GigabitEthernet0/0/23       auto         1     1-4094

[LSW2]nt eth
[LSW2]int eth-
[LSW2]int Eth-Trunk 1
[LSW2-Eth-Trunk1]port lik
[LSW2-Eth-Trunk1]port lin
[LSW2-Eth-Trunk1]port link-type trunk
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW2-Eth-Trunk1]q
[LSW2]ping 192.168.10.3
  PING 192.168.10.3: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out
    Request time out
    Request time out
    Request time out

  --- 192.168.10.3 ping statistics ---
    5 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW2]dis port vlan
Port                        Link Type    PVID  Trunk VLAN List
-------------------------------------------------------------------------------
Eth-Trunk1                  trunk        1     1
GigabitEthernet0/0/1        access       1     -
GigabitEthernet0/0/2        access       1     -
GigabitEthernet0/0/3        -            0     -
GigabitEthernet0/0/4        -            0     -
GigabitEthernet0/0/5        -            0     -
GigabitEthernet0/0/6        auto         1     1-4094
GigabitEthernet0/0/7        auto         1     1-4094
GigabitEthernet0/0/8        auto         1     1-4094
GigabitEthernet0/0/9        auto         1     1-4094
GigabitEthernet0/0/10       auto         1     1-4094
GigabitEthernet0/0/11       auto         1     1-4094
GigabitEthernet0/0/12       auto         1     1-4094
GigabitEthernet0/0/13       auto         1     1-4094
GigabitEthernet0/0/14       auto         1     1-4094
GigabitEthernet0/0/15       auto         1     1-4094
GigabitEthernet0/0/16       auto         1     1-4094
GigabitEthernet0/0/17       auto         1     1-4094
GigabitEthernet0/0/18       auto         1     1-4094
GigabitEthernet0/0/19       auto         1     1-4094
GigabitEthernet0/0/20       auto         1     1-4094
GigabitEthernet0/0/21       auto         1     1-4094
GigabitEthernet0/0/22       auto         1     1-4094
GigabitEthernet0/0/23       auto         1     1-4094

[LSW2]int Eth-Trunk 1
[LSW2-Eth-Trunk1]port trunk al
[LSW2-Eth-Trunk1]port trunk allow-pass all
                                       ^
Error: Unrecognized command found at '^' position.
[LSW2-Eth-Trunk1]port trunk allow-pass vlan a
[LSW2-Eth-Trunk1]port trunk allow-pass vlan all
Info: This operation may take a few seconds. Please wait a moment.done.
[LSW2-Eth-Trunk1]q
[LSW2]ping 192.168.10.3
  PING 192.168.10.3: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out

  --- 192.168.10.3 ping statistics ---
    2 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW2]dis port vlan
Port                        Link Type    PVID  Trunk VLAN List
-------------------------------------------------------------------------------
Eth-Trunk1                  trunk        1     1-4094
GigabitEthernet0/0/1        access       1     -
GigabitEthernet0/0/2        access       1     -
GigabitEthernet0/0/3        -            0     -
GigabitEthernet0/0/4        -            0     -
GigabitEthernet0/0/5        -            0     -
GigabitEthernet0/0/6        auto         1     1-4094
GigabitEthernet0/0/7        auto         1     1-4094
GigabitEthernet0/0/8        auto         1     1-4094
GigabitEthernet0/0/9        auto         1     1-4094
GigabitEthernet0/0/10       auto         1     1-4094
GigabitEthernet0/0/11       auto         1     1-4094
GigabitEthernet0/0/12       auto         1     1-4094
GigabitEthernet0/0/13       auto         1     1-4094
GigabitEthernet0/0/14       auto         1     1-4094
GigabitEthernet0/0/15       auto         1     1-4094
GigabitEthernet0/0/16       auto         1     1-4094
GigabitEthernet0/0/17       auto         1     1-4094
GigabitEthernet0/0/18       auto         1     1-4094
GigabitEthernet0/0/19       auto         1     1-4094
GigabitEthernet0/0/20       auto         1     1-4094
GigabitEthernet0/0/21       auto         1     1-4094
GigabitEthernet0/0/22       auto         1     1-4094
GigabitEthernet0/0/23       auto         1     1-4094

[LSW2]ping 192.168.10.3
  PING 192.168.10.3: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out

  --- 192.168.10.3 ping statistics ---
    2 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW2]ping 192.168.10.2
  PING 192.168.10.2: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out
    Request time out
    Request time out
    Request time out

  --- 192.168.10.2 ping statistics ---
    5 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW2]int g0/0/1
[LSW2-GigabitEthernet0/0/1]port default vl
[LSW2-GigabitEthernet0/0/1]port default vlan 10
[LSW2-GigabitEthernet0/0/1]q
[LSW2]int g0/0/2
[LSW2-GigabitEthernet0/0/2]port default vlan 20
[LSW2-GigabitEthernet0/0/2]q
[LSW2]ping 192.168.20.1
  PING 192.168.20.1: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out

  --- 192.168.20.1 ping statistics ---
    2 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW2]ping 192.168.20.2
  PING 192.168.20.2: 56  data bytes, press CTRL_C to break
    Request time out
    Request time out

  --- 192.168.20.2 ping statistics ---
    2 packet(s) transmitted
    0 packet(s) received
    100.00% packet loss

[LSW2]dis port vlan
Port                        Link Type    PVID  Trunk VLAN List
-------------------------------------------------------------------------------
Eth-Trunk1                  trunk        1     1-4094
GigabitEthernet0/0/1        access       10    -
GigabitEthernet0/0/2        access       20    -
GigabitEthernet0/0/3        -            0     -
GigabitEthernet0/0/4        -            0     -
GigabitEthernet0/0/5        -            0     -
GigabitEthernet0/0/6        auto         1     1-4094
GigabitEthernet0/0/7        auto         1     1-4094
GigabitEthernet0/0/8        auto         1     1-4094
GigabitEthernet0/0/9        auto         1     1-4094
GigabitEthernet0/0/10       auto         1     1-4094
GigabitEthernet0/0/11       auto         1     1-4094
GigabitEthernet0/0/12       auto         1     1-4094
GigabitEthernet0/0/13       auto         1     1-4094
GigabitEthernet0/0/14       auto         1     1-4094
GigabitEthernet0/0/15       auto         1     1-4094
GigabitEthernet0/0/16       auto         1     1-4094
GigabitEthernet0/0/17       auto         1     1-4094
GigabitEthernet0/0/18       auto         1     1-4094
GigabitEthernet0/0/19       auto         1     1-4094
GigabitEthernet0/0/20       auto         1     1-4094
GigabitEthernet0/0/21       auto         1     1-4094
GigabitEthernet0/0/22       auto         1     1-4094
GigabitEthernet0/0/23       auto         1     1-4094

[LSW2]
[LSW2]dis vlan
The total number of VLANs is: 3
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
1    common  UT:GE0/0/6(D)      GE0/0/7(D)      GE0/0/8(D)      GE0/0/9(D)
                GE0/0/10(D)     GE0/0/11(D)     GE0/0/12(D)     GE0/0/13(D)
                GE0/0/14(D)     GE0/0/15(D)     GE0/0/16(D)     GE0/0/17(D)
                GE0/0/18(D)     GE0/0/19(D)     GE0/0/20(D)     GE0/0/21(D)
                GE0/0/22(D)     GE0/0/23(D)     GE0/0/24(D)     GE0/0/25(D)
                GE0/0/26(D)     GE0/0/27(D)     GE0/0/28(D)     Eth-Trunk1(U)
10   common  UT:GE0/0/1(U)
             TG:Eth-Trunk1(U)
20   common  UT:GE0/0/2(U)
             TG:Eth-Trunk1(U)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
1    enable  default       enable  disable    VLAN 0001
10   enable  default       enable  disable    VLAN 0010
20   enable  default       enable  disable    VLAN 0020
[LSW2]disp int vlanif 10
                      ^
Error: Wrong parameter found at '^' position.
[LSW2]

User interface con0 is available

Please Press ENTER.

Login authentication

Username:admin
Password:
Info: Lastest accessed IP: Invalid IP address  Time: 2024-11-30 14:31:51  Failed: 0

Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommended version information.
<LSW2>dis eth
<LSW2>dis eth-trunk 1
Eth-Trunk1's state information is:
Local:
LAG ID: 1                   WorkingMode: LACP
Preempt Delay: Disabled     Hash arithmetic: According to SIP-XOR-DIP
System Priority: 32768      System ID: 6012-3c9a-61f0
Least Active-linknumber: 1  Max Active-linknumber: 8
Operate status: up          Number Of Up Port In Trunk: 2
--------------------------------------------------------------------------------
ActorPortName          Status   PortType PortPri PortNo PortKey PortState Weight
GigabitEthernet0/0/3   Selected 1GE      32768   1      305     10111100  1
GigabitEthernet0/0/4   Selected 1GE      32768   2      305     10111100  1
GigabitEthernet0/0/5   Unselect 1GE      32768   3      305     10110000  1

Partner:
--------------------------------------------------------------------------------
ActorPortName          SysPri   SystemID        PortPri PortNo PortKey PortState
GigabitEthernet0/0/3   100      642c-acc1-65e0  100     1      305     10111100
GigabitEthernet0/0/4   100      642c-acc1-65e0  100     2      305     10111100
GigabitEthernet0/0/5   100      642c-acc1-65e0  32768   3      305     10100000

<LSW2>

User interface con0 is available

Please Press ENTER.