[LSW1-aaa]
[LSW1-aaa]q
[LSW1]disp vlan
The total number of VLANs is: 1
--------------------------------------------------------------------------------
U: Up;         D: Down;         TG: Tagged;         UT: Untagged;
MP: Vlan-mapping;               ST: Vlan-stacking;
#: ProtocolTransparent-vlan;    *: Management-vlan;
--------------------------------------------------------------------------------

VID  Type    Ports
--------------------------------------------------------------------------------
1    common  UT:GE0/0/1(U)      GE0/0/2(U)      GE0/0/3(D)      GE0/0/4(D)
                GE0/0/5(D)      GE0/0/6(D)      GE0/0/7(D)      GE0/0/8(D)
                GE0/0/9(D)      GE0/0/10(D)     GE0/0/11(D)     GE0/0/12(D)
                GE0/0/13(D)     GE0/0/14(D)     GE0/0/15(D)     GE0/0/16(D)
                GE0/0/17(D)     GE0/0/18(D)     GE0/0/19(D)     GE0/0/20(D)
                GE0/0/21(D)     GE0/0/22(D)     GE0/0/23(U)     GE0/0/24(D)
                GE0/0/25(D)     GE0/0/26(D)     GE0/0/27(D)     GE0/0/28(D)

VID  Status  Property      MAC-LRN Statistics Description
--------------------------------------------------------------------------------
1    enable  default       enable  disable    VLAN 0001
[LSW1]disp int vlanif 10
Vlanif10 current state : DOWN
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet Address is 10.10.10.20/24
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 6012-3c9a-5ffb
Current system time: 2024-12-05 14:19:44
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

[LSW1]disp int vlanif 100
                      ^
Error: Wrong parameter found at '^' position.
[LSW1]disp int vlanif 20
                      ^
Error: Wrong parameter found at '^' position.
[LSW1]disp int vlanif all
                      ^
Error: Wrong parameter found at '^' position.
[LSW1]disp int vlanif
Vlanif1 current state : UP
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet protocol processing : disabled
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 6012-3c9a-5ff2
Current system time: 2024-12-05 14:19:55
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

Vlanif10 current state : DOWN
Line protocol current state : DOWN
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet Address is 10.10.10.20/24
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 6012-3c9a-5ffb
Current system time: 2024-12-05 14:19:55
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

[LSW1]int g0/0/23
[LSW1-GigabitEthernet0/0/23]vlan 10
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW1-vlan10]dis this
#
return
[LSW1-vlan10]int g0/0/23
[LSW1-GigabitEthernet0/0/23]port de
[LSW1-GigabitEthernet0/0/23]port default vlan 10
[LSW1-GigabitEthernet0/0/23]port link
[LSW1-GigabitEthernet0/0/23]port link-t
[LSW1-GigabitEthernet0/0/23]port link-type trunk
Warning: This command will delete VLANs on this port. Continue?[Y/N]:n
[LSW1-GigabitEthernet0/0/23]q
[LSW1]dis vlanif 10
          ^
Error: Unrecognized command found at '^' position.
[LSW1]dis int vlanif 10
Vlanif10 current state : UP
Line protocol current state : UP
Last line protocol up time : 2024-12-05 14:21:04
Description:
Route Port,The Maximum Transmit Unit is 1500
Internet Address is 10.10.10.20/24
IP Sending Frames' Format is PKTFMT_ETHNT_2, Hardware address is 6012-3c9a-5ffb
Current system time: 2024-12-05 14:21:31
    Input bandwidth utilization  : --
    Output bandwidth utilization : --

[LSW1]save
           ^
Error:Incomplete command found at '^' position.
[LSW1]commit
      ^
Error: Unrecognized command found at '^' position.
[LSW1]
[SwitchA]
[SwitchA]stp mode stp
[SwitchA]
[LSW1]
[LSW1]
[LSW1]
[LSW1]
[LSW1]

Login authentication

Username:
#Easy-Operation: Stop upgrading because of the input in the console.
#Easy-Operation: Enter the status of running normally.admin
Password:
Error: Authentication fail

Username:admin
Password:
Warning: The default password poses security risks.
The password needs to be changed. Change now? [Y/N]: y
Please enter old password:
Please enter new password:
Please confirm new password:
The password has been changed successfully.
Info: Lastest accessed IP: Invalid IP address  Time: 2024-12-05 14:32:10  Failed                                                                  : 1

Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommend                                                                  ed version information.
<HUAWEI>sys
Enter system view, return user view with Ctrl+Z.
[HUAWEI]sysname LSW2
[LSW2]
Dec  5 2024 14:32:46 LSW2 DS/4/DATASYNC_CFGCHANGE:OID 1.3.6.1.4.1.2011.5.25.191.                                                                  3.1 configurations have been changed. The current change number is 238, the chan                                                                  ge loop count is 0, and the maximum number of records is 4095.
[LSW2]un in en
Info: Information center is disabled.
[LSW2]
[LSW2]
[LSW2]stp mode stp
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW2]stp bpdu-protection
[LSW2]stp pathcost-standard legacy
Info: This operation may take a few seconds. Please wait for a moment...done.
Warning: The path cost of the current process will be set to the default value b                                                                  ecause the path cost standard is changed.
[LSW2]int g0/0/2
[LSW2-GigabitEthernet0/0/2] stp edged-port enable
[LSW2-GigabitEthernet0/0/2]return
<LSW2>
<LSW2>sys
[LSW2] stp enable
[LSW2]q
<LSW2>

Login authentication

Username:
#Easy-Operation: Stop upgrading because of the input in the console.
#Easy-Operation: Enter the status of running normally.
Username:admin
Password:
Warning: The default password poses security risks.
The password needs to be changed. Change now? [Y/N]: y
Please enter old password:
Please enter new password:
Please confirm new password:
The password has been changed successfully.
Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommend                                                                  ed version information.
<HUAWEI>sys
Enter system view, return user view with Ctrl+Z.
[HUAWEI]sysname LSW3
[LSW3]
Dec  5 2024 14:33:44 LSW3 DS/4/DATASYNC_CFGCHANGE:OID 1.3.6.1.4.1.2011.5.25.191.                                                                  3.1 configurations have been changed. The current change number is 242, the chan                                                                  ge loop count is 0, and the maximum number of records is 4095.
[LSW3]stp mode stp
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW3]stp bpdu-protection
Dec  5 2024 14:33:49 LSW3 %%01MSTP/4/SET_PORT_DISCARDING(l)[0]:In MSTP process 0                                                                   instance 0, MSTP set port GigabitEthernet0/0/1 state as discarding.
Dec  5 2024 14:33:49 LSW3 %%01MSTP/4/SET_PORT_DISCARDING(l)[1]:In MSTP proc
[LSW3]stp pathcost-standard legacyess 0 instance 0, MSTP set port GigabitEtherne                                                                  t0/0/2 state as discarding.
Dec  5 2024 14:33:49 LSW3 %%01MSTP/4/SET_PORT_DISCARDING(l)[2]:In MSTP process 0                                                                   instance 0, MSTP set port GigabitEthernet0/0/3 state as discarding.
[LSW3]stp pathcost-standard legacy
Dec  5 2024 14:33:50 LSW3 %%01MSTP/4/SET_PORT_DISCARDING(l)[3]:In MSTP process 0                                                                   instance 0, MSTP set port GigabitEthernet0/0/3 state as discarding.
[LSW3]stp pathcost-standard legacy
Info: This operation may take a few seconds. Please wait for a moment...done.
Warning: The path cost of the current process will be set to the default value b                                                                  ecause the path cost standard is changed.
[LSW3]
Dec  5 2024 14:33:54 LSW3 DS/4/DATASYNC_CFGCHANGE:OID 1.3.6.1.4.1.2011.5.25.191.                                                                  3.1 configurations have been changed. The current change number is 245, the chan                                                                  ge loop count is 0, and the maximum number of records is 4095.
[LSW3]un in en
Info: Information center is disabled.
[LSW3]stp mode stp
[LSW3]stp bpdu-protection
[LSW3]stp pathcost-standard legacy
[LSW3]int g0/0/1
[LSW3-GigabitEthernet0/0/1]stp instance 0 cost 20000
[LSW3-GigabitEthernet0/0/1]int g0/0/3
[LSW3-GigabitEthernet0/0/3]int g0/0/2
[LSW3-GigabitEthernet0/0/2] stp edged-port enable
[LSW3-GigabitEthernet0/0/2]return
<LSW3>

Login authentication

Username:
#Easy-Operation: Stop upgrading because of the input in the console.
#Easy-Operation: Enter the status of running normally.admin
Password:
Warning: The default password poses security risks.
The password needs to be changed. Change now? [Y/N]: y
Please enter old password:
Please enter new password:
Please confirm new password:
The password has been changed successfully.
Info: Smart-upgrade is currently disabled. Enable Smart-upgrade to get recommend                                                                  ed version information.
<HUAWEI>sys
Enter system view, return user view with Ctrl+Z.
[HUAWEI]sysname LSW4
[LSW4]
Dec  5 2024 14:35:46 LSW4 DS/4/DATASYNC_CFGCHANGE:OID 1.3.6.1.4.1.2011.5.25.191.                                                                  3.1 configurations have been changed. The current change number is 242, the chan                                                                  ge loop count is 0, and the maximum number of records is 4095.
[LSW4]un in en
Info: Information center is disabled.
[LSW4]#
[LSW4]stp mode stp
Info: This operation may take a few seconds. Please wait for a moment...done.
[LSW4]stp instance 0 root secondary
[LSW4]stp pathcost-standard legacy
Info: This operation may take a few seconds. Please wait for a moment...done.
Warning: The path cost of the current process will be set to the default value b                                                                  ecause the path cost standard is changed.
[LSW4]#
[LSW4]return
<LSW4>

User interface con0 is available

Please Press ENTER.