Script started on Tue Jun 16 15:36:06 2020
bash-4.2$ make test
sh ./C1377.sh
mcstop+release.sh ... done
mcreboot.sh -c 1-7,9-15,17-23,25-31 -m 10G@0,10G@1 -r 1-7:0+9-15:8+17-23:16+25-31:24 ... done
*** C1377T01 start
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
..................................................
*** C1377T01 PASS ok: 1000
wait02      1  TPASS  :  wait(&status) returned 32240
*** C1377T02: wait02 PASS (1)
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
wait401.c:55: PASS: waitpid() returned correct pid 32347
wait401.c:64: PASS: WIFEXITED() is set in status
wait401.c:69: PASS: WEXITSTATUS() == 0

Summary:
passed   3
failed   0
skipped  0
warnings 0
*** C1377T03: wait401 PASS (3)
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
waitpid01.c:51: PASS: waitpid() returned correct pid 32454
waitpid01.c:60: PASS: WIFSIGNALED() set in status
waitpid01.c:68: PASS: WTERMSIG() == SIGALRM

Summary:
passed   3
failed   0
skipped  0
warnings 0
*** C1377T04: waitpid01 PASS (3)
waitpid02    1  TPASS  :  received expected pid
waitpid02    2  TPASS  :  received expected signal
waitpid02    3  TPASS  :  received expected exit value
*** C1377T05: waitpid02 PASS (3)
waitpid04    1  TPASS  :  condition 1 test passed
waitpid04    2  TPASS  :  condition 2 test passed
waitpid04    3  TPASS  :  condition 3 test passed
*** C1377T06: waitpid04 PASS (3)
waitpid05    1  TPASS  :  received expected pid.
waitpid05    2  TPASS  :  received expected exit number.
waitpid05    3  TPASS  :  received expected pid.
waitpid05    4  TPASS  :  received expected exit number.
waitpid05    5  TPASS  :  received expected pid.
waitpid05    6  TPASS  :  received expected exit number.
waitpid05    7  TPASS  :  received expected pid.
waitpid05    8  TPASS  :  received expected exit number.
waitpid05    9  TPASS  :  received expected pid.
waitpid05   10  TPASS  :  received expected exit number.
waitpid05   11  TPASS  :  received expected pid.
waitpid05   12  TPASS  :  received expected exit number.
waitpid05   13  TPASS  :  received expected pid.
waitpid05   14  TPASS  :  received expected exit number.
waitpid05   15  TPASS  :  received expected pid.
waitpid05   16  TPASS  :  received expected exit number.
waitpid05   17  TPASS  :  received expected pid.
waitpid05   18  TPASS  :  received expected exit number.
waitpid05   19  TPASS  :  received expected pid.
waitpid05   20  TPASS  :  received expected exit number.
waitpid05   21  TPASS  :  received expected pid.
waitpid05   22  TPASS  :  received expected exit number.
waitpid05   23  TPASS  :  received expected pid.
waitpid05   24  TPASS  :  received expected exit number.
*** C1377T07: waitpid05 PASS (24)
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
waitpid06.c:54: PASS: Test PASSED

Summary:
passed   1
failed   0
skipped  0
warnings 0
*** C1377T08: waitpid06 PASS (1)
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
waitpid07.c:59: PASS: Test PASSED

Summary:
passed   1
failed   0
skipped  0
warnings 0
*** C1377T09: waitpid07 PASS (1)
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
waitpid_common.h:142: INFO: Sending SIGCONT to 1524
waitpid_common.h:142: INFO: Sending SIGCONT to 1554
waitpid_common.h:142: INFO: Sending SIGCONT to 1584
waitpid_common.h:142: INFO: Sending SIGCONT to 1614
waitpid_common.h:142: INFO: Sending SIGCONT to 1644
waitpid_common.h:142: INFO: Sending SIGCONT to 1674
waitpid_common.h:142: INFO: Sending SIGCONT to 1704
waitpid_common.h:142: INFO: Sending SIGCONT to 1734
waitpid08.c:62: PASS: Test PASSED

Summary:
passed   1
failed   0
skipped  0
warnings 0
*** C1377T10: waitpid08 PASS (1)
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
waitpid09.c:83: PASS: waitpid(pid, WNOHANG) = 0 for a running child
waitpid09.c:123: PASS: waitpid(pid, WNOHANG) = pid for an exited child
waitpid09.c:143: PASS: waitpid(-1, 0) = -1 with ECHILD if no children
waitpid09.c:162: PASS: waitpid(-1, WNOHANG) = -1 with ECHILD if no children

Summary:
passed   4
failed   0
skipped  0
warnings 0
*** C1377T11: waitpid09 PASS (4)
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
waitpid10.c:62: PASS: Test PASSED

Summary:
passed   1
failed   0
skipped  0
warnings 0
*** C1377T12: waitpid10 PASS (1)
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
waitpid11.c:60: PASS: Test PASSED

Summary:
passed   1
failed   0
skipped  0
warnings 0
*** C1377T13: waitpid11 PASS (1)
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
waitpid12.c:70: PASS: Test PASSED

Summary:
passed   1
failed   0
skipped  0
warnings 0
*** C1377T14: waitpid12 PASS (1)
tst_test.c:1096: INFO: Timeout per run is 0h 05m 00s
waitpid_common.h:142: INFO: Sending SIGCONT to 6219
waitpid_common.h:142: INFO: Sending SIGCONT to 6249
waitpid_common.h:142: INFO: Sending SIGCONT to 6279
waitpid_common.h:142: INFO: Sending SIGCONT to 6309
waitpid_common.h:142: INFO: Sending SIGCONT to 6099
waitpid_common.h:142: INFO: Sending SIGCONT to 6129
waitpid_common.h:142: INFO: Sending SIGCONT to 6159
waitpid_common.h:142: INFO: Sending SIGCONT to 6189
waitpid13.c:70: PASS: Test PASSED

Summary:
passed   1
failed   0
skipped  0
warnings 0
*** C1377T15: waitpid13 PASS (1)
bash-4.2$ exit
exit

Script done on Tue Jun 16 15:55:52 2020
