*** C1025T01 ******************************************
** Linux's result *************************************
[type: HARDWARE, counter: HW_REF_CPU_CYCLES, exclude: none]
REF_CPU_CYCLES         :         48755980
[type: HARDWARE, counter: HW_REF_CPU_CYCLES, exclude: user]
REF_CPU_CYCLES         :           153686
[type: HARDWARE, counter: HW_REF_CPU_CYCLES, exclude: kernel]
REF_CPU_CYCLES         :         48527830

** McKernel's result *************************************
[type: HARDWARE, counter: HW_REF_CPU_CYCLES, exclude: none]
REF_CPU_CYCLES         :         48341332
[type: HARDWARE, counter: HW_REF_CPU_CYCLES, exclude: user]
REF_CPU_CYCLES         :            32584
[type: HARDWARE, counter: HW_REF_CPU_CYCLES, exclude: kernel]
REF_CPU_CYCLES         :         48403544
check user val: 48403544 is IN 43675047.0 - 53380613.0 [OK]
check kernel val: 32584 is IN 0 - 484035.44 [OK]
** C1025T01 PASSED

*** C1025T02 ******************************************
** Linux's result *************************************
[ CASE-A , Leader fd : YES , exclude: none]
REF_CPU_CYCLES         :         48236994
CPU_CYCLES             :         48235903
[ CASE-A , Leader fd : YES , exclude: user]
REF_CPU_CYCLES         :           164606
CPU_CYCLES             :           163696
[ CASE-A , Leader fd : YES , exclude: kernel]
REF_CPU_CYCLES         :         48176180
CPU_CYCLES             :         48176171

** McKernel's result *************************************
[ CASE-A , Leader fd : YES , exclude: none]
REF_CPU_CYCLES         :         48159124
CPU_CYCLES             :         48158854
[ CASE-A , Leader fd : YES , exclude: user]
REF_CPU_CYCLES         :            33256
CPU_CYCLES             :            34166
[ CASE-A , Leader fd : YES , exclude: kernel]
REF_CPU_CYCLES         :         48114404
CPU_CYCLES             :         48113129
check user val: 48114404 is IN 43358562.0 - 52993798.0 [OK]
check kernel val: 33256 is IN 0 - 481144.04 [OK]
** C1025T02 PASSED

*** C1025T03 ******************************************
** Linux's result *************************************
[ CASE-B , Leader fd : YES , exclude: none]
REF_CPU_CYCLES         :         48421568
CPU_CYCLES             :         48420573
[ CASE-B , Leader fd : YES , exclude: user]
REF_CPU_CYCLES         :           150592
CPU_CYCLES             :           149560
[ CASE-B , Leader fd : YES , exclude: kernel]
REF_CPU_CYCLES         :         48131044
CPU_CYCLES             :         48131051

** McKernel's result *************************************
[ CASE-B , Leader fd : YES , exclude: none]
REF_CPU_CYCLES         :         48218332
CPU_CYCLES             :         48217927
[ CASE-B , Leader fd : YES , exclude: user]
REF_CPU_CYCLES         :            26588
CPU_CYCLES             :            27440
[ CASE-B , Leader fd : YES , exclude: kernel]
REF_CPU_CYCLES         :         48184988
CPU_CYCLES             :         48183719
check user val: 48184988 is IN 43317939.6 - 52944148.4 [OK]
check kernel val: 26588 is IN 0 - 481849.88 [OK]
** C1025T03 PASSED

*** C1025T04 ******************************************
** Linux's result *************************************
[ CASE-C , Leader fd : YES , exclude: none]
REF_CPU_CYCLES         :                0
CPU_CYCLES             :                0
[ CASE-C , Leader fd : YES , exclude: user]
REF_CPU_CYCLES         :                0
CPU_CYCLES             :                0
[ CASE-C , Leader fd : YES , exclude: kernel]
REF_CPU_CYCLES         :                0
CPU_CYCLES             :                0

** McKernel's result *************************************
[ CASE-C , Leader fd : YES , exclude: none]
REF_CPU_CYCLES         :                0
CPU_CYCLES             :                0
[ CASE-C , Leader fd : YES , exclude: user]
REF_CPU_CYCLES         :                0
CPU_CYCLES             :                0
[ CASE-C , Leader fd : YES , exclude: kernel]
REF_CPU_CYCLES         :                0
CPU_CYCLES             :                0
check user val: 0 is IN 0 - 0 [OK]
check kernel val: 0 is IN 0 - 0 [OK]
** C1025T04 PASSED

*** C1025T05 ******************************************
** Linux's result *************************************
[ CASE-D , Leader fd : YES , exclude: none]
** Result of 1st read
REF_CPU_CYCLES         :         48435452
CPU_CYCLES             :         48434766
** Result of 2nd read
REF_CPU_CYCLES         :         96713214
CPU_CYCLES             :         96712309
[ CASE-D , Leader fd : YES , exclude: user]
** Result of 1st read
REF_CPU_CYCLES         :           167726
CPU_CYCLES             :           167090
** Result of 2nd read
REF_CPU_CYCLES         :           218972
CPU_CYCLES             :           217925
[ CASE-D , Leader fd : YES , exclude: kernel]
** Result of 1st read
REF_CPU_CYCLES         :         48358310
CPU_CYCLES             :         48358416
** Result of 2nd read
REF_CPU_CYCLES         :         96665374
CPU_CYCLES             :         96665155

** McKernel's result *************************************
[ CASE-D , Leader fd : YES , exclude: none]
** Result of 1st read
REF_CPU_CYCLES         :         48349424
CPU_CYCLES             :         48350565
** Result of 2nd read
REF_CPU_CYCLES         :         96533776
CPU_CYCLES             :         96534029
[ CASE-D , Leader fd : YES , exclude: user]
** Result of 1st read
REF_CPU_CYCLES         :           120252
CPU_CYCLES             :           123202
** Result of 2nd read
REF_CPU_CYCLES         :           124820
CPU_CYCLES             :           127588
[ CASE-D , Leader fd : YES , exclude: kernel]
** Result of 1st read
REF_CPU_CYCLES         :         48220612
CPU_CYCLES             :         48218625
** Result of 2nd read
REF_CPU_CYCLES         :         96400228
CPU_CYCLES             :         96397658
check user val 1st: 48220612 is IN 43522479.0 - 53194141.0 [OK]
check kernel val 1st: 120252 is IN 0 - 482206.12 [OK]
check user val 2nd: 96400228 is IN 86998836.6 - 106331911.4 [OK]
check kernel val 2nd: 124820 is IN 0 - 964002.28 [OK]
** C1025T05 PASSED

*** C1025T06 ******************************************
** Linux's result *************************************
[ CASE-E , Leader fd : YES , exclude: none]
REF_CPU_CYCLES         :         96772780
CPU_CYCLES             :         96770849
[ CASE-E , Leader fd : YES , exclude: user]
REF_CPU_CYCLES         :           266708
CPU_CYCLES             :           264912
[ CASE-E , Leader fd : YES , exclude: kernel]
REF_CPU_CYCLES         :         96471518
CPU_CYCLES             :         96471732

** McKernel's result *************************************
[ CASE-E , Leader fd : YES , exclude: none]
REF_CPU_CYCLES         :         96521304
CPU_CYCLES             :         96520373
[ CASE-E , Leader fd : YES , exclude: user]
REF_CPU_CYCLES         :            28396
CPU_CYCLES             :            29419
[ CASE-E , Leader fd : YES , exclude: kernel]
REF_CPU_CYCLES         :         96486100
CPU_CYCLES             :         96484240
check user val: 96486100 is IN 86824366.2 - 106118669.8 [OK]
check kernel val: 28396 is IN 0 - 964861.00 [OK]
** C1025T06 PASSED

*** C1025T07 ******************************************
** Linux's result *************************************
[ CASE-F , Leader fd : YES , exclude: none]
REF_CPU_CYCLES         :         97312774
CPU_CYCLES             :         97311964
[ CASE-F , Leader fd : YES , exclude: user]
REF_CPU_CYCLES         :           217334
CPU_CYCLES             :           216399
[ CASE-F , Leader fd : YES , exclude: kernel]
REF_CPU_CYCLES         :         96420454
CPU_CYCLES             :         96420276

** McKernel's result *************************************
[ CASE-F , Leader fd : YES , exclude: none]
REF_CPU_CYCLES         :         96623504
CPU_CYCLES             :         96624703
[ CASE-F , Leader fd : YES , exclude: user]
REF_CPU_CYCLES         :           122824
CPU_CYCLES             :           129819
[ CASE-F , Leader fd : YES , exclude: kernel]
REF_CPU_CYCLES         :         96483264
CPU_CYCLES             :         96483351
check user val: 96483264 is IN 86778408.6 - 106062499.4 [OK]
check kernel val: 122824 is IN 0 - 964832.64 [OK]
** C1025T07 PASSED

*** C1025T08 ******************************************
** Linux's result *************************************
[ CASE-A , Leader fd : NO , exclude: none]
CPU_CYCLES             :         48327271
REF_CPU_CYCLES         :         48326278
[ CASE-A , Leader fd : NO , exclude: user]
CPU_CYCLES             :           181571
REF_CPU_CYCLES         :           180544
[ CASE-A , Leader fd : NO , exclude: kernel]
CPU_CYCLES             :         48163955
REF_CPU_CYCLES         :         48163934

** McKernel's result *************************************
[ CASE-A , Leader fd : NO , exclude: none]
CPU_CYCLES             :         48155129
REF_CPU_CYCLES         :         48155124
[ CASE-A , Leader fd : NO , exclude: user]
CPU_CYCLES             :            35583
REF_CPU_CYCLES         :            34760
[ CASE-A , Leader fd : NO , exclude: kernel]
CPU_CYCLES             :         48127029
REF_CPU_CYCLES         :         48128300
check user val: 48128300 is IN 43347540.6 - 52980327.4 [OK]
check kernel val: 34760 is IN 0 - 481283.00 [OK]
** C1025T08 PASSED

*** C1025T09 ******************************************
** Linux's result *************************************
[ CASE-B , Leader fd : NO , exclude: none]
CPU_CYCLES             :         48449221
REF_CPU_CYCLES         :         48448270
[ CASE-B , Leader fd : NO , exclude: user]
CPU_CYCLES             :           155589
REF_CPU_CYCLES         :           154544
[ CASE-B , Leader fd : NO , exclude: kernel]
CPU_CYCLES             :         48160727
REF_CPU_CYCLES         :         48160710

** McKernel's result *************************************
[ CASE-B , Leader fd : NO , exclude: none]
CPU_CYCLES             :         48217557
REF_CPU_CYCLES         :         48218028
[ CASE-B , Leader fd : NO , exclude: user]
CPU_CYCLES             :            31206
REF_CPU_CYCLES         :            30500
[ CASE-B , Leader fd : NO , exclude: kernel]
CPU_CYCLES             :         48185577
REF_CPU_CYCLES         :         48186852
check user val: 48186852 is IN 43344639.0 - 52976781.0 [OK]
check kernel val: 30500 is IN 0 - 481868.52 [OK]
** C1025T09 PASSED

*** C1025T10 ******************************************
** Linux's result *************************************
[ CASE-C , Leader fd : NO , exclude: none]
CPU_CYCLES             :                0
REF_CPU_CYCLES         :                0
[ CASE-C , Leader fd : NO , exclude: user]
CPU_CYCLES             :                0
REF_CPU_CYCLES         :                0
[ CASE-C , Leader fd : NO , exclude: kernel]
CPU_CYCLES             :                0
REF_CPU_CYCLES         :                0

** McKernel's result *************************************
[ CASE-C , Leader fd : NO , exclude: none]
CPU_CYCLES             :                0
REF_CPU_CYCLES         :                0
[ CASE-C , Leader fd : NO , exclude: user]
CPU_CYCLES             :                0
REF_CPU_CYCLES         :                0
[ CASE-C , Leader fd : NO , exclude: kernel]
CPU_CYCLES             :                0
REF_CPU_CYCLES         :                0
check user val: 0 is IN 0 - 0 [OK]
check kernel val: 0 is IN 0 - 0 [OK]
** C1025T10 PASSED

*** C1025T11 ******************************************
** Linux's result *************************************
[ CASE-D , Leader fd : NO , exclude: none]
** Result of 1st read
CPU_CYCLES             :         48495513
REF_CPU_CYCLES         :         48494706
** Result of 2nd read
CPU_CYCLES             :         96769906
REF_CPU_CYCLES         :         96768906
[ CASE-D , Leader fd : NO , exclude: user]
** Result of 1st read
CPU_CYCLES             :           167295
REF_CPU_CYCLES         :           166634
** Result of 2nd read
CPU_CYCLES             :           218489
REF_CPU_CYCLES         :           217958
[ CASE-D , Leader fd : NO , exclude: kernel]
** Result of 1st read
CPU_CYCLES             :         48240264
REF_CPU_CYCLES         :         48240270
** Result of 2nd read
CPU_CYCLES             :         96429199
REF_CPU_CYCLES         :         96429060

** McKernel's result *************************************
[ CASE-D , Leader fd : NO , exclude: none]
** Result of 1st read
CPU_CYCLES             :         48432773
REF_CPU_CYCLES         :         48433336
** Result of 2nd read
CPU_CYCLES             :         96650562
REF_CPU_CYCLES         :         96651624
[ CASE-D , Leader fd : NO , exclude: user]
** Result of 1st read
CPU_CYCLES             :           134833
REF_CPU_CYCLES         :           133472
** Result of 2nd read
CPU_CYCLES             :           139726
REF_CPU_CYCLES         :           138260
[ CASE-D , Leader fd : NO , exclude: kernel]
** Result of 1st read
CPU_CYCLES             :         48218540
REF_CPU_CYCLES         :         48220536
** Result of 2nd read
CPU_CYCLES             :         96397701
REF_CPU_CYCLES         :         96400280
check user val 1st: 48220536 is IN 43416243.0 - 53064297.0 [OK]
check kernel val 1st: 133472 is IN 0 - 482205.36 [OK]
check user val 2nd: 96400280 is IN 86786154.0 - 106071966.0 [OK]
check kernel val 2nd: 138260 is IN 0 - 964002.80 [OK]
** C1025T11 PASSED

*** C1025T12 ******************************************
** Linux's result *************************************
[ CASE-E , Leader fd : NO , exclude: none]
CPU_CYCLES             :         97011286
REF_CPU_CYCLES         :         97009406
[ CASE-E , Leader fd : NO , exclude: user]
CPU_CYCLES             :           218390
REF_CPU_CYCLES         :           216502
[ CASE-E , Leader fd : NO , exclude: kernel]
CPU_CYCLES             :         96375684
REF_CPU_CYCLES         :         96375526

** McKernel's result *************************************
[ CASE-E , Leader fd : NO , exclude: none]
CPU_CYCLES             :         96511772
REF_CPU_CYCLES         :         96512684
[ CASE-E , Leader fd : NO , exclude: user]
CPU_CYCLES             :            28379
REF_CPU_CYCLES         :            27540
[ CASE-E , Leader fd : NO , exclude: kernel]
CPU_CYCLES             :         96484648
REF_CPU_CYCLES         :         96486504
check user val: 96486504 is IN 86737973.4 - 106013078.6 [OK]
check kernel val: 27540 is IN 0 - 964865.04 [OK]
** C1025T12 PASSED

*** C1025T13 ******************************************
** Linux's result *************************************
[ CASE-F , Leader fd : NO , exclude: none]
CPU_CYCLES             :         96528511
REF_CPU_CYCLES         :         96527652
[ CASE-F , Leader fd : NO , exclude: user]
CPU_CYCLES             :           209363
REF_CPU_CYCLES         :           208832
[ CASE-F , Leader fd : NO , exclude: kernel]
CPU_CYCLES             :         96227150
REF_CPU_CYCLES         :         96226858

** McKernel's result *************************************
[ CASE-F , Leader fd : NO , exclude: none]
CPU_CYCLES             :         96505364
REF_CPU_CYCLES         :         96505988
[ CASE-F , Leader fd : NO , exclude: user]
CPU_CYCLES             :            80671
REF_CPU_CYCLES         :            75140
[ CASE-F , Leader fd : NO , exclude: kernel]
CPU_CYCLES             :         96369863
REF_CPU_CYCLES         :         96369692
check user val: 96369692 is IN 86604172.2 - 105849543.8 [OK]
check kernel val: 75140 is IN 0 - 963696.92 [OK]
** C1025T13 PASSED

